# Assembling the saw stand (see figures A1−A2)

Carefully remove all parts included in the delivery from their packaging.
Remove all packing material.

- Place the folded base frame (2) flat on the floor.
- Pull up the base frame (2) by the unlocking lever (1).
  Let go of the unlocking lever whilst pulling it up so the saw stand can click into place.
- Insert the saw stand legs (3) into the square pipes in the base frame (2) until they are aligned with the assembly holes.
- Screw together the saw stand legs and the base frame using the nuts and bolts in the fastening set (4).