# Extending the saw table

The free end of long and heavy workpieces must have something placed underneath it or be supported.

##

The saw table expansion (11) increases the width of the saw table (17) on the right.

- Pull the clamping handle (18) for the saw table expansion all the way up.
- Pull out the saw table expansion (11) to the required length.
- Push the clamping handle (18) down. This fixes the saw table expansion in place.

##

The saw table extension (10) increases the length of the saw table (17) to the rear.

- Loosen the locking screw (38) on the left guide rod.
- Pull out the saw table extension (10) to the required length.
- To fix it in position, tighten the locking screw (38).

You may need to support the saw table extension when working with heavy workpieces.

##

The slide carriage (2) makes it possible to saw workpieces up to a maximum width of 350 mm.
It also ensures greater sawing precision, in particular when used in connection with the angle guide (3) see Sawing mitre angles using the slide carriage.

- Pull the clamping handle (29) for the slide carriage all the way up.
  This makes it possible to move the slide carriage all the way to the front or back.