# Product features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Scale for spacing between saw blade and parallel guide
(2) | Slide carriage
(3) | Angle guide
(4) | Carrying handle
(5) | Label for marking the cutting line
(6) | Protective cover
(7) | Riving knife
(8) | Parallel guide
(9) | Guide groove for angle guide
(10) | Saw table extension
(11) | Saw table expansion
(12) | Securing nut for the saw blade storage compartment cover and for hanging the push stick
(13) | Push stick
(14) | Saw blade storage compartment cover
(15) | Ring spanner (24 mm; 23 mm)
(16) | Mounting holes
(17) | Saw table
(18) | Clamping handle for saw table expansion
(19) | Hand wheel
(20) | Crank for raising and lowering the saw blade
(21) | Safety flap for the on/off switch
(22) | Bracket for storing the protective cover
(23) | Holding clip for storing the angle guide
(24) | Guide bar of the saw table extension
(25) | Stop for 45° bevel angle
(26) | Locking lever for setting the bevel angle
(27) | Scale for bevel angles
(28) | Stop for 0° bevel angle
(29) | Clamping handle for slide carriage
(30) | V guide groove on the saw table for the parallel guide
(31) | Adjusting screw for adjusting the clamping force of the parallel guide
(32) | Table insert
(33) | Saw blade
(34) | Profile rail
(35) | Guide groove for parallel guide
(36) | Parallel guide storage compartment
(37) | Hex key (5 mm)
(38) | Locking screw of the saw table extension
(39) | "Additional parallel guide" fastening set
(40) | Chip ejector
(41) | Dust extraction adapter
(42) | Cable holder
(43) | "Saw table extension" fastening set
(44) | V guide for parallel guide
(45) | Base plate
(46) | Clamping lever for riving knife
(47) | Positioning pins for riving knife
(48) | Recesses for table insert
(49) | Clamping lever for protective cover
(50) | Guide pin for protective cover
(51) | Clamping handle for parallel guide
(52) | Additional parallel guide
(53) | Guide rail for angle guide
(54) | Knurled screw for fixing the angle guide
(55) | "Profile rail" fastening set
(56) | Knurled nut for profile rail
(57) | Lower saw blade cover
(58) | Fastening screw of the lower saw blade cover
(59) | Clamping nut
(60) | Spindle locking lever
(61) | Clamping flange
(62) | Mounting flange
(63) | Tool spindle
(64) | Angle indicator (vertical)
(65) | Locking knob for all mitre angles
(66) | Mitre angle indicator on the angle guide
(67) | Adjusting plate
(68) | Magnifying glass
(69) | Saw table spacing indicator
(70) | On button
(71) | Cross-head screw for setting the 0° stop
(72) | Screw for bevel angle indicator
(73) | Cross-head screw for setting the 45° stop
(74) | Hex socket screws (5 mm) on the front for adjusting the parallelism of the saw blade
(75) | Hex socket screws (5 mm) on the rear for adjusting the parallelism of the saw blade
(76) | Screw for saw table spacing indicator
(77) | Hex socket screws (5 mm) for adjusting the parallelism of the parallel guide
(78) | Screw for parallel guide spacing indicator
(79) | Adjusting screws for table insert
(80) | Bracket for storing the "additional parallel guide" fastening set
(81) | Holding clip for storing the dust extraction adapter
(82) | Saw blade storage compartment
(83) | Bracket for storing the hex key
(84) | Holding clip for storing the additional parallel guide