# Maintenance and Cleaning

- Pull the plug out of the socket before carrying out any work on the power tool.

- To ensure safe and efficient operation, always keep the power tool and the ventilation slots clean.

In order to avoid safety hazards, if the power supply cord needs to be replaced, this must be done by Bosch or by an after-sales service centre that is authorised to repair Bosch power tools.

##

Always remove dust and chips after working by blowing out with compressed air or using a brush.

##

Lubricant:
SAE 10/SAE 20 engine oil

- Oil the power tool as necessary at the points indicated (see figure S).

An authorised Bosch after-sales service point will handle this work quickly and reliably.

- Dispose of lubricants and cleaning products in an environmentally friendly manner, taking legal regulations into account.

##

Measures implemented by the manufacturer:

- Soft start
- Provided with a saw blade specially developed for noise reduction

Measures implemented by the operator:

- Low-vibration mounting on a stable work surface
- Use of saw blades with noise-reducing functions
- Regular cleaning of the saw blade and power tool