# Storage and transport

## Storing tool elements (see figures R1–R6)

You can attach certain tool elements to the power tool to store them.

- Detach the additional parallel guide (52) from the parallel guide (8).
- Place all loose components of the tool in their storage compartments on the housing (see the following table).

Figure | Tool element | Storage compartment
--- | --- | ---
R1 | Protective cover (6) | Place in the recess on the bracket (22) and secure using the clamping lever (49)
R2 | "Additional parallel guide" fastening set (39) | Clip into the brackets (80)
R2 | Dust extraction adapter (41) | Slide into the holding clips (81)
R3 | Unused saw blades | Place in the saw blade storage compartment (82) and fasten the cover (14) above it with the securing nut (12)
R3 | Ring spanner (15) | Place in the saw blade storage compartment (82) and fasten the cover (14) above it with the securing nut (12)
R3 | Push stick (13) | Attach with the securing nut (12)
R4 | Hex key (37) | Slide into the brackets (83)
R4 | Parallel guide (8) | Place in the parallel guide storage compartment (36)
R5 | Angle guide (3) | Slide into the holding clips (23)
R6 | Additional parallel guide (52) | Place in the additional parallel guide storage compartment and secure with the holding clip (84)

## Transporting the power tool

Before transporting the power tool, the following steps must be carried out:

- Bring the power tool into the transport position.
- Remove all accessories that cannot be securely fitted to the power tool.
  If possible, transport unused saw blades in an enclosed container.
- Slide the saw table expansion (11) in fully and push the clamping handle (18) downwards to secure it in place.
- Slide the saw table extension (10) all the way in and tighten the locking screws (38) on the guide bars (24).
- Wrap the power cable around the cable holder (42).
- Use the carrying handles (4) to lift or transport the tool.

- Only use the transport devices to transport the power tool and never the protective devices.