# Technical data

Table saw |  | GTS 10 XC | GTS 10 XC | GTS 10 XC
--- | --- | --- | --- | ---
Article number |  | ‎3 601 M30 403 ‎3 601 M30 473 | ‎3 601 M30 432 | ‎3 601 M30 462
Rated power input | W | 2000 | 2000 | 1650
Rated voltage | V | 220–240 | 230 | 110
Frequency | Hz | 50–60 | 50–60 | 50–60
No-load speed | min–1 | 4200 | 4200 | 4200
Starting current limitation |  | ● | ● | ●
Run-out brake |  | ● | ● | ●
Overload protection |  | ● | ● | ●
Weight according to EPTA-Procedure 01:2014 | kg | 35.0 | 35.0 | 35.0
Protection class |  | / II | / II | / II
Dimensions (including detachable parts of the tool)
Width x depth x height | mm | 783 x 771 x 343 | 783 x 771 x 343 | 783 x 771 x 343
Dimensions of suitable saw blades
Saw blade diameter | mm | 254 | 254 | 254
Base blade thickness | mm | < 2.2 | < 2.2 | < 2.2
Min. tooth thickness/offset | mm | > 2.4 | > 2.4 | > 2.4
Hole diameter | mm | 30 | 30 | 30

Table saw |  | GTS 10 XC | GTS 10 XC
--- | --- | --- | ---
Article number |  | ‎3 601 M30 443 | ‎3 601 M30 4B3
Rated power input | W | 2000 | 2000
Rated voltage | V | 220–240 | 220
Frequency | Hz | 50–60 | 60
No-load speed | min–1 | 4200 | 4200
Starting current limitation |  | ● | ●
Run-out brake |  | ● | ●
Overload protection |  | ● | ●
Weight according to EPTA-Procedure 01:2014 | kg | 35.0 | 35.0
Protection class |  | / II | / II
Dimensions (including detachable parts of the tool)
Width x depth x height | mm | 783 x 771 x 343 | 783 x 771 x 343
Dimensions of suitable saw blades
Saw blade diameter | mm | 254 | 254
Base blade thickness | mm | < 2.2 | < 2.2
Min. tooth thickness/offset | mm | > 2.4 | > 2.4
Hole diameter | mm | 25.4 | 25.4

Maximum workpiece dimensions: see Maximum workpiece dimensions

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.