# Symbols

The following symbols may be important for the operation of your power tool. Please take note of these symbols and their meaning. Correctly interpreting the symbols will help you to operate the power tool more effectively and safely.

Symbols and their meaning
| Keep hands away from the cutting area while the power tool is running. Contact with the saw blade can lead to injuries.
| Wear a dust mask.
| Wear hearing protection. Exposure to noise can cause hearing loss.
| Wear safety goggles.
‎3 601 M30 502‎ ‎3 601 M30 532‎ ‎3 601 M30 562‎ ‎3 601 M30 572‎ ‎3 601 M30 542‎ ‎3 601 M30 5B2 | Observe the dimensions of the saw blade. The hole diameter must match the tool spindle without play. If it is necessary to use reducers, ensure that the dimensions of the reducer are suitable for the base blade thickness and the saw blade hole diameter, as well as the tool spindle diameter. Wherever possible, use the reducers provided with the saw blade. The saw blade diameter must match the information specified on the symbol.
| a The saw blade must be no more than 254 mm in diameter. b The riving knife is 2.3 mm thick. c The cutting direction of the teeth (direction of the arrow on the saw blade) must match the direction of the arrow on the riving knife. d When changing the saw blade, make sure that the cutting width is no smaller than 2.4 mm and the base blade thickness is no larger than 2.2 mm. Otherwise, there is a risk that the riving knife will hook into the workpiece.
| The riving knife is 2.3 mm thick. The maximum possible workpiece height is 79 mm.
| Left-hand side: Indicates the direction of rotation of the crank for lowering (transport position) and raising (work position) the saw blade. Right-hand side: Indicates the position of the locking lever for securing the saw blade and setting the bevel angle (saw blade can be swivelled).
| Oil the power tool as necessary at the points indicated.
| Protection class II power tools are strengthened or double-insulated.
| The CE mark provides confirmation from the manufacturer that the power tool complies with the applicable EU Directives.