# Items included

Check to ensure that all the parts listed below have been supplied before using the power tool for the first time:

- Table saw with fitted saw blade (26) and riving knife (7)
- Angle guide (3)
- Profile rail (28)
- "Profile rail" fastening set (44) (guide plate, knurled nut, screw, washer)
- Parallel guide (9)
- Additional parallel guide (41)
- "Additional parallel guide" fastening set (42) (3 fastening screws, 3 washers, 3 wing nuts)
- Protective cover (6)
- Hex key (21)
- Hex key (20)
- Ring spanner (22)
- Push stick (23)
- Table insert (25)
- Dust extraction adapter (32)

Note: Check the power tool for possible damage.
Before continuing to use the power tool, carefully check that all protective devices or slightly damaged parts are working perfectly and according to specifications. Check that the moving parts are working perfectly and without jamming; check whether any parts are damaged. All parts must be fitted correctly and all the conditions necessary to ensure smooth operation must be met.
If the protective devices or any parts become damaged, you must have them properly repaired or replaced by an authorised service centre.