# Storage and transport

## Storing tool elements (see figures O1–O5)

You can attach certain tool elements to the power tool to store them.

- Detach the additional parallel guide (41) from the parallel guide (9).
- Place all loose components of the tool in their storage compartments on the housing (see the following table).

Figure | Tool element | Storage compartment
--- | --- | ---
O1 | Protective cover | Place in the recess on the bracket (33) and secure using the clamping lever (37)
O2 | "Additional parallel guide" fastening set (42) | Clip into the brackets (69)
O2 | Dust extraction adapter (32) | Slide into the holding clips (70)
O3 | Ring spanner (22) | Secure in the storage compartment using the securing nut (71)
O3 | Push stick (23) | Suspend using the securing nut (71) and slide to secure
O4 | Parallel guide (9) | Turn around, suspend from below in the guide rails and secure the clamping handle (39)
O5 | Hex key (21) Hex key (20) | Slide into the brackets (72)
O5 | Angle guide (3) | Slide into the holding clips (73)
O5 | Additional parallel guide (41) | Slide into the holding clips (30) (short side facing up, long side facing the rear)

## Transporting the power tool

Before transporting the power tool, the following steps must be carried out:

- Bring the power tool into the transport position.
- Remove all accessories that cannot be securely fitted to the power tool.
  If possible, transport unused saw blades in an enclosed container.
- Slide the saw table expansion (13) in fully and push the clamping handle (15) down to secure it in place.
- Wrap the power cable around the cable holder (29).
- Use the carrying handles (12) to lift or transport the tool.

- Only use the transport devices to transport the power tool and never the protective devices.