# Product features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Guide groove for parallel guide
(2) | Scale for spacing between saw blade and parallel guide
(3) | Angle guide
(4) | Recessed handles
(5) | Guide groove for angle guide
(6) | Protective cover
(7) | Riving knife
(8) | Saw table
(9) | Parallel guide
(10) | V guide groove on the saw table for the parallel guide
(11) | Mounting holes
(12) | Carrying handle
(13) | Saw table expansion
(14) | Fixing clip for the GTA 600 saw stand
(15) | Clamping handle for saw table expansion
(16) | Locking lever for setting the bevel angle
(17) | Hand wheel
(18) | Crank for raising and lowering the saw blade
(19) | On/off switch safety flap
(20) | Hex key (2 mm)
(21) | Hex key (5 mm)
(22) | Ring spanner (23 mm)
(23) | Push stick
(24) | Adjusting screw for adjusting the clamping force of the parallel guide
(25) | Table insert
(26) | Saw blade
(27) | Magnifying glass
(28) | Profile rail
(29) | Cable holder
(30) | Holding clip for storing the additional parallel guide
(31) | Chip ejector
(32) | Dust extraction adapter
(33) | Bracket for storing the protective cover
(34) | Clamping lever for riving knife
(35) | Positioning pins for riving knife
(36) | Recesses for table insert
(37) | Clamping lever for protective cover
(38) | Guide pin for protective cover
(39) | Clamping handle of the parallel guide
(40) | V guide of the parallel guide
(41) | Additional parallel guide
(42) | "Additional parallel guide" fastening set
(43) | Guide rail of the angle guide
(44) | "Profile rail" fastening set
(45) | Fastening screw for chip ejector
(46) | Clamping nut
(47) | Spindle locking lever
(48) | Clamping flange
(49) | Tool spindle
(50) | Mounting flange
(51) | Bevel angle indicator
(52) | Scale for bevel angles
(53) | Locking knob for all mitre angles
(54) | Angle indicator on the angle guide
(55) | Saw table spacing indicator
(56) | On button
(57) | Knurled nut for profile rail
(58) | Cross-head screw for setting the 0° stop
(59) | Stop for 0° bevel angle
(60) | Screw for bevel angle indicator
(61) | Cross-head screw for setting the 45° stop
(62) | Stop for 45° bevel angle
(63) | Hex socket screws (5 mm) on the front for adjusting the parallelism of the saw blade
(64) | Hex socket screws (5 mm) on the rear for adjusting the parallelism of the saw blade
(65) | Screw for saw table spacing indicator
(66) | Hex socket screws (5 mm) for adjusting the parallelism of the parallel guide
(67) | Screw for parallel guide spacing indicator
(68) | Adjusting screws for table insert
(69) | Bracket for storing the "additional parallel guide" fastening set
(70) | Holding clip for storing the dust extraction adapter
(71) | Securing nut for the ring spanner and for hanging the push stick
(72) | Bracket for storing the hex key
(73) | Holding clip for storing the angle guide