# Technical data

Table saw |  | GTS 10 J | GTS 10 J | GTS 10 J
--- | --- | --- | --- | ---
Article number |  | ‎3 601 M30 502‎ ‎3 601 M30 572‎ | ‎3 601 M30 532‎ | ‎3 601 M30 562‎
Rated power input | W | 1800 | 1800 | 1650
Rated voltage | V | 220–240 | 230 | 110
Frequency | Hz | 50/60 | 50/60 | 50/60
No-load speed | min-1 | 3650 | 3650 | 3650
Starting current limitation |  | ● | ● | ●
Weight according to EPTA-Procedure 01:2014 | kg | 26.2 | 26.2 | 26.2
Protection class |  | / II | / II | / II
Dimensions (including detachable parts of the tool)
Width x depth x height | mm | 640 x 706 x 330 | 640 x 706 x 330 | 640 x 706 x 330
Dimensions of suitable saw blades
Saw blade diameter | mm | 254 | 254 | 254
Base blade thickness | mm | < 2.2 | < 2.2 | < 2.2
Min. tooth thickness/offset | mm | > 2.4 | > 2.4 | > 2.4
Hole diameter | mm | 30 | 30 | 30

Table saw |  | GTS 10 J | GTS 10 J
--- | --- | --- | ---
Article number |  | ‎3 601 M30 542‎ | ‎3 601 M30 5B2
Rated power input | W | 1800 | 1800
Rated voltage | V | 220–240 | 220
Frequency | Hz | 50/60 | 60
No-load speed | min-1 | 3650 | 3650
Starting current limitation |  | ● | ●
Weight according to EPTA-Procedure 01:2014 | kg | 26.2 | 26.2
Protection class |  | / II | / II
Dimensions (including detachable parts of the tool)
Width x depth x height | mm | 640 x 706 x 330 | 640 x 706 x 330
Dimensions of suitable saw blades
Saw blade diameter | mm | 254 | 254
Base blade thickness | mm | < 2.2 | < 2.2
Min. tooth thickness/offset | mm | > 2.4 | > 2.4
Hole diameter | mm | 25.4 | 25.4

Maximum workpiece dimensions: see Maximum workpiece dimensions

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.

The appliance meets IEC 61000-3-11 requirements and is subject to conditional connection. The appliance can lead to occasional voltage fluctuations under unfavorable power conditions. The impedance of this appliance is set as Zactual = 0.048 Ω. The user must make sure, that the connection point, with the impedance Zmax, on which the appliance shall be plugged in meets the impedance requirement: Zactual ≥ Zmax. If Zmax is unknown, determine Zmax in consultation with the network supplier or supply authority.