# Additional safety warnings

- When mounting the saw blade, wear protective gloves. This poses a risk of injury.

- Do not use HSS saw blades. Such saw blades can easily break.

- Only use saw blades that match the specifications given in this operating manual and that are tested and marked in accordance with EN 847-1

- Never use the tool without the table insert. Replace table insert if defective. Without flawless table inserts, injuries are possible from the saw blade.

- Keep your work area clean. Material mixtures are particularly hazardous. Light metal dust may catch fire or explode.

- Choose the saw blade suited to the material you want to work on.

- Only use saw blades that are recommended by the power tool manufacturer and are suitable for using on the material you want to saw.

- Only advance the workpiece towards the saw blade when it is running. Otherwise there is a risk of kickback occurring if the saw blade catches in the workpiece.

Products sold in GB only:

Your product is fitted with an BS 1363/A approved electric plug with internal fuse (ASTA approved to BS 1362).

If the plug is not suitable for your socket outlets, it should be cut off and an appropriate plug fitted in its place by an authorised customer service agent. The replacement plug should have the same fuse rating as the original plug.

The severed plug must be disposed of to avoid a possible shock hazard and should never be inserted into a mains socket elsewhere.