# Storage and transport

## Storing tool elements (see figures O1 – O2)

You can attach certain tool elements to the power tool to store them.

- Detach the additional parallel guide (41) from the parallel guide (5).
- Place all loose components of the tool in their storage compartments on the housing (see the following table).

Tool element | Storage compartment
--- | ---
Parallel guide (5) | Turn around, suspend from below in the guide rails and secure the clamping handle (39)
Push stick (12) | Place in the storage compartment (68)
Protective cover (3) | Place in the recess on the bracket (11) and secure using the clamping lever (37)
Hex key (10) | Place in the storage compartment (69)
Ring spanner (9) | Place in the storage compartment (70)
Angle guide (2) | Place in the storage compartment (7)
Additional parallel guide (41) | Push into the groove at the back of the parallel guide (5) and tighten using the wing bolts

## Transporting the power tool

Before transporting the power tool, the following steps must be carried out:

- Bring the power tool into the transport position.
- Remove all accessories that cannot be securely fitted to the power tool.
  If possible, transport unused saw blades in an enclosed container.
- Slide the saw table expansion (6) in fully and push the clamping handle (13) down to secure it in place.
- Wrap the power cable around the cable holder (26).
- Use the carrying handles (27) to lift or transport the tool.

- Only use the transport devices to transport the power tool and never the protective devices.