# Product Features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Scale for spacing between saw blade and parallel guide
(2) | Angle guide
(3) | Protective cover
(4) | Riving knife
(5) | Parallel guide
(6) | Saw table expansion
(7) | Angle guide storage compartment
(8) | Mounting holes
(9) | Ring spanner (23 mm; 13 mm)
(10) | Hex key (5 mm)
(11) | Bracket for storing the protective cover
(12) | Push stick
(13) | Clamping handle for saw table expansion
(14) | Hand wheel
(15) | Crank for raising and lowering the saw blade
(16) | On/off switch
(17) | BatteryA)
(18) | Stop for 45° bevel angle
(19) | Scale for bevel angles
(20) | Locking lever for setting the bevel angle
(21) | Angle indicator (vertical)
(22) | Stop for 0° bevel angle
(23) | Saw table
(24) | Adjusting screw for adjusting the clamping force of the parallel guide
(25) | Table insert
(26) | Saw blade
(27) | Guide groove for parallel guide
(28) | Battery release buttonA)
(29) | Carrying handle
(30) | Guide groove for angle guide
(31) | Dust extraction adapter
(32) | V guide groove on the saw table for the parallel guide
(33) | Base grid
(34) | Locking screw for base grid
(35) | Clamping lever/clamp markings
(36) | Clamping lever for riving knife
(37) | Positioning pins for riving knife
(38) | Table insert locking screw
(39) | Clamping lever for protective cover
(40) | Guide pin for protective cover
(41) | Clamping handle for parallel guide
(42) | V guide for parallel guide
(43) | Additional parallel guide
(44) | "Additional parallel guide" fastening set
(45) | Guide rail for angle guide
(46) | Lower saw blade cover
(47) | Tab for lower saw blade cover
(48) | Gripping hole for lifting the table insert
(49) | Clamping nut
(50) | Spindle locking lever
(51) | Clamping flange
(52) | Mounting flange
(53) | Tool spindle
(54) | Locking knob for all mitre angles
(55) | Angle indicator on the angle guide
(56) | Scale display
(57) | Saw table spacing indicator
(58) | Cross-head screw for setting the 0° stop
(59) | Screw for bevel angle indicator
(60) | Cross-head screw for setting the 45° stop
(61) | Hex socket screws (5 mm) on the front for adjusting the parallelism of the saw blade
(62) | Hex socket screws (5 mm) on the rear for adjusting the parallelism of the saw blade
(63) | Screw for saw table spacing indicator
(64) | Hex socket screws (5 mm) for adjusting the parallelism of the parallel guide
(65) | Screw for parallel guide spacing indicator
(66) | Adjusting screws for table insert
(67) | Push stick storage compartment
(68) | Hex key storage compartment
(69) | Ring spanner storage compartment

A)

  Accessories shown or described are not included with the product as standard. You can find the complete selection of accessories in our accessories range.