# Transport position and work position of the saw blade

## Transport position

- Remove the protective cover (3), remove the table insert (25) and place the riving knife (4) in the bottom position. Reinsert the table insert (25).
- Turn the crank (15) anticlockwise until the teeth of the saw blade (26) lie below the saw table (23).
- Push the saw table expansion (6) in fully.
  Push the clamping handle (13) down. This fixes the saw table expansion in place.

## Work position

- Position the riving knife (4) in the top position directly over the centre of the saw blade, insert the table insert (25) and fit the protective cover (3).
- Turn the crank (15) clockwise until the top teeth of the saw blade (26) are approx. 3−6 mm above the workpiece.