# Additional safety warnings

- When mounting the saw blade, wear protective gloves. This poses a risk of injury.

- Do not use HSS saw blades. Such saw blades can easily break.

- Only use saw blades that match the specifications given in this operating manual and that are tested and marked in accordance with EN 847-1

- Never use the tool without the table insert. Replace table insert if defective. Without flawless table inserts, injuries are possible from the saw blade.

- Keep your work area clean. Material mixtures are particularly hazardous. Light metal dust may catch fire or explode.

- Choose the saw blade suited to the material you want to work on.

- Only use saw blades that are recommended by the power tool manufacturer and are suitable for using on the material you want to saw.

- Only advance the workpiece towards the saw blade when it is running. Otherwise there is a risk of kickback occurring if the saw blade catches in the workpiece.

- In case of damage and improper use of the battery, vapours may be emitted. The battery can set alight or explode. Ensure the area is well ventilated and seek medical attention should you experience any adverse effects. The vapours may irritate the respiratory system.

- Do not open the battery. There is a risk of short-circuiting.

- The battery can be damaged by pointed objects such as nails or screwdrivers or by force applied externally. An internal short circuit may occur, causing the battery to burn, smoke, explode or overheat.

- Only use the battery with products from the manufacturer. This is the only way in which you can protect the battery against dangerous overload.

| Protect the battery against heat, e.g. against continuous intense sunlight, fire, dirt, water and moisture. There is a risk of explosion and short-circuiting.