# Adjusting the parallel guide

The parallel guide (5) can be positioned on either the left (black scale) or the right (silver scale) of the saw blade. The marking in the scale display (56) shows the set distance between the parallel guide and the saw blade on the scale (1).
Position the parallel guide on the required side of the saw blade see Fitting the parallel guide (see figure e).

## Adjusting the parallel guide
when the saw table is not pulled out

- Loosen the clamping handle (41) of the parallel guide (5). Move the parallel guide until the marking in the scale display (56) indicates the required distance from the saw blade.
  When the saw table is not pulled out, the lower marking on the silver scale (1) applies.
- To secure it in place, push the clamping handle (41) back down.

## Adjusting the parallel guide
when the saw table is pulled out (see figure D)

- Position the parallel guide on the right of the saw blade.
  Move the parallel guide until the marking in the scale display (56) shows 29 cm on the lower scale.
  To secure it in place, push the clamping handle (41) back down.
- Pull the clamping handle (13) for the saw table expansion all the way up.
- Pull out the saw table expansion (6) until the spacing indicator (57) shows the required distance from the saw blade on the upper scale.
- Push the clamping handle (13) down.
  This fixes the saw table expansion in place.