# Storage and transport

## Storing tool elements (see figures O1 – O2)

You can attach certain tool elements to the power tool to store them.

- Detach the additional parallel guide (43) from the parallel guide (5).
- Place all loose components of the tool in their storage compartments on the housing (see the following table).

Tool element | Storage compartment
--- | ---
Parallel guide (5) | Turn around, suspend from below in the guide rails and secure the clamping handle (41)
Push stick (12) | Place in the storage compartment (67)
Protective cover (3) | Place in the recess on the bracket (11) and secure using the clamping lever (39)
Hex key (10) | Place in the storage compartment (68)
Ring spanner (9) | Place in the storage compartment (69)
Angle guide (2) | Place in the storage compartment (7)
Additional parallel guide (43) | Push into the groove at the back of the parallel guide (5) and tighten using the wing bolts

## Transporting the power tool

- Remove the battery from the power tool before carrying out work on the power tool (e.g. maintenance, changing tool, etc.). The battery should also be removed for transport and storage. There is risk of injury from unintentionally pressing the on/off switch.

Before transporting the power tool, the following steps must be carried out:

- Bring the power tool into the transport position see Transport position.
- Remove all accessories that cannot be securely fitted to the power tool.
  If possible, transport unused saw blades in a closed container.
- Slide the saw table expansion (6) in fully and push the clamping handle (13) downwards to secure it in place.
- Use the carrying handles (29) to lift or transport the tool.

- Only use the transport devices to transport the power tool and never the protective devices.