# Operation

- Remove the battery from the power tool before carrying out work on the power tool (e.g. maintenance, changing tool, etc.). The battery should also be removed for transport and storage. There is risk of injury from unintentionally pressing the on/off switch.

Transport position and work position of the saw blade
Extending the saw table
Setting mitre and bevel angles
Adjusting the parallel guide
Adjusting the Additional Parallel Guide
Adjusting the riving knife
Start-up
Practical advice
Sawing
Checking and adjusting the basic settings
Storage and transport