# Changing the saw blade (see figures l1−l4)

- Remove the battery from the power tool before carrying out work on the power tool (e.g. maintenance, changing tool, etc.). The battery should also be removed for transport and storage. There is risk of injury from unintentionally pressing the on/off switch.

- When mounting the saw blade, wear protective gloves. This poses a risk of injury.

- Only use saw blades the maximum permitted speed of which is higher than the no-load speed of the power tool.

- Only use saw blades that match the specifications given in this operating manual and that are tested and marked in accordance with EN 847-1

- Only use saw blades that are recommended by the power tool manufacturer and are suitable for use on the material you want to saw. This prevents the saw tooth tips from overheating and the plastic you want to saw from melting.

- Do not use HSS saw blades. Such saw blades can easily break.

##

- Open the clamping lever (39) and pull the protective cover (3) out of the groove on the riving knife (4).
- Turn the locking screw (38) as far as possible in the "Unlock" direction using the tip of the ring spanner (9) and lift the table insert (25) out of the tool chamber. A gripping hole (48) is integrated into the tool for ease of lifting.
- Turn the crank (15) clockwise as far as possible so that the saw blade (26) is in the highest possible position above the saw table.
- Turn the clamping nut (49) using the ring spanner (9) while pulling the spindle locking lever (50) until it engages.
- Keep pulling the spindle locking lever and unscrew the clamping nut anticlockwise.
- Remove the clamping flange (51).
- Remove the saw blade (26).

##

- If necessary, clean all the parts you want to fit before installing them.
- Place the new saw blade on the mounting flange (52) of the tool spindle (53).

Note: Use sufficiently large saw blades. The radial clearance between the saw blade and the riving knife must not exceed 3−8 mm (max.).

- When fitting the saw blade, make sure that the cutting direction of the teeth (direction of the arrow on the saw blade) matches the direction of the arrow on the riving knife.

- Fit the clamping flange (51) and the clamping nut (49).
- Turn the clamping nut (49) using the ring spanner (9) while pulling the spindle locking lever (50) until it engages.
- Tighten the clamping nut by turning it clockwise.
- Place the table insert (25) over the riving knife (4) and into the tool chamber. Turn the locking screw (38) as far as it will go in the "Lock" direction using the tip of the ring spanner (9).
- Refit the protective cover (3) .