# Technical Data

Table saw |  | GTS 18V-216 | GTS 18V-216
--- | --- | --- | ---
Article number |  | ‎3 601 M44 000 ‎3 601 M44 040 ‎3 601 M44 0K0 | ‎3 601 M44 0B0
Rated voltage | V= | 18 | 18
No-load speedA) | min-1 | 4500 | 4500
Starting current limitation |  | ● | ●
Weight according to EPTA-Procedure 01:2014B) | kg | 20.5−21.6 | 20.5−21.6
Recommended ambient temperature during charging | °C | 0...+35 | 0...+35
Permitted ambient temperature during operationC) and during storage | °C | –20...+50 | –20...+50
Compatible rechargeable batteries |  | GBA 18V... ProCORE18V... | GBA 18V... ProCORE18V...
Recommended rechargeable batteries for maximum performance |  | ProCORE18V... ≥ 5.5 Ah | ProCORE18V... ≥ 5.5 Ah
Recommended chargers |  | GAL 18... GAX 18... GAL 36... | GAL 18... GAX 18... GAL 36...
Dimensions (including detachable parts of the tool)
Width x depth x height | mm | 658 x 332 x 553 | 658 x 332 x 553
Dimensions of suitable saw blades
Saw blade diameter | mm | 216 | 216
Base blade thickness | mm | <1.5 | 1.5–2.1
Min. tooth thickness/offset | mm | >1.7 | >2.3
Hole diameter | mm | 30 | 25.4

A)

  Measured at 20–25 °C with rechargeable battery ProCORE18V 12.0Ah.

B)

  Depends on battery in use

C)

  Limited performance at temperatures < 0 °C

Maximum workpiece dimensions: see Maximum workpiece dimensions

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.