# Practical advice

##

Two laser beams indicate the cutting width of the saw blade. This allows for exact positioning of the workpiece for sawing, without having to open the retracting blade guard.

- Switch on the laser beams with the switch (6).
- Position your mark on the workpiece between the two laser lines.

Note: Before sawing, check if the cutting width is still indicated correctly see Adjusting the laser. Vibrations during intensive use, for example, can cause the laser beams to become misaligned.

##

Maximum workpiece dimensions:

Mitre angle | Bevel angle | Height x width [mm]
--- | --- | ---
0° | 0° | 70 x 305
45° (left/right) | 0° | 70 x 215
45° (left) | 45° (left) | 42 x 215
45° (right) | 45° (right) | 20 x 215
0° | 45° (left) | 42 x 305
0° | 45° (right) | 20 x 305

Minimum workpiece dimensions (= all workpieces that can be secured left or right of the saw blade using the supplied screw clamps (41)): 100 x 40 mm (length x width)

Maximum cutting depth (0°/0°): 70 mm

##

The depth stop needs to be adjusted if you wish to saw a groove.

- Swivel the depth stop (39) forwards.
- Swivel the tool arm by the handle (9) into the required position.
- Turn the adjusting screw (38) until the end of the screw touches the depth stop (39).
- Slowly guide the tool arm upwards.

##

The left or right length stop (36) can be used for easily sawing workpieces of the same length.

- Turn the length stop (36) upwards.
- Set the saw table extension (25) to the required workpiece length.

##

When sawing curved or round workpieces, these must be especially secured against slipping. At the cutting line, there should be no gap between the workpiece, fence and saw table.

If necessary, you will need to manufacture special fixtures.

##

The insert plates (16) can become worn after prolonged use of the power tool.

Replace faulty insert plates.

- Bring the power tool into the work position.
- Unscrew the screws (54) using a commercially available cross-headed screwdriver and remove the old insert plate (16).
- Insert the new insert plate and screw the screws (54) in tight again.