# Fitting individual components

- Carefully remove all parts included in the delivery from their packaging.
- Remove all packing material from the power tool and the accessories provided.

- For ease of assembly when fitting the tool elements that are provided, be aware that the power tool is supplied in the transport position.

##

The workpiece supports (26) can be positioned left, right or in front of the power tool. The flexible connector system enables a multitude of extension or expansion variants (see figure G).

- Insert the workpiece support (26) into the openings (47) on the power tool or into the openings (48) of the second workpiece support as required.

- Never carry the power tool using the workpiece supports.
  Only use the transport devices to transport the power tool.

##

The clamping wheel (45) fixes the selected bevel angle and is required for safe operation.

- Unscrew the hex nut from the threaded bolts (49).
- Screw the clamping wheel (45) clockwise onto the threaded bolts (49) and tighten it.

##

The adjustable fence (28) must be fitted before sawing.

- Slide the fence (28) on the right of the saw blade into the corresponding groove and tighten the locking screw (44).
  The levelled side of the fence must face inwards towards the saw blade.