# Adjusting bevel angles

The bevel angle can be set between 47° (left-hand side) and 47° (right-hand side).

For quick and precise setting of frequently used bevel angles, fixed positions have been provided for the angles 0°, 22.5° and 45°.

- Make sure that the clamping wheel (45) is fitted see Fitting the Clamping Wheel (see figure A2).

## Setting Standard Bevel Angles (see figure L)

- Pull the adjustable fences (28) all the way out or remove them completely.
- Release the clamping wheel (45).
- Pull the locking lever (46) out and engage it in the free running position.
  This enables you to use the complete bevel angle range (left and right).
- Swivel the tool arm left or right by the handle (9) until the angle indicator (30) shows the required standard bevel angle.
- Turn the locking lever (46). The locking lever must be felt to engage in the position of the required standard bevel angle.
- Retighten the clamping wheel (45).

## Setting any bevel angle

- Pull the adjustable fences (28) all the way out or remove them completely.
- Release the clamping wheel (45).
- Pull the locking lever (46) out and engage it in the free running position.
  This enables you to use the complete bevel angle range (left and right).
- Swivel the tool arm left or right by the handle (9) until the angle indicator (30) shows the required bevel angle.
- Retighten the clamping wheel (45).