# Symbols

## Europe

The following symbols may be important for the operation of your power tool. Please take note of these symbols and their meaning. Correctly interpreting the symbols will help you to operate the power tool more effectively and safely.

Symbols and their meaning
| Laser radiation Do not look directly into the beam Class 2 consumer laser product EN 50689:2021
| Keep hands away from the cutting area while the power tool is running. Contact with the saw blade can lead to injuries.
| Wear a dust mask.
| Wear safety goggles.
| Wear hearing protection. Exposure to noise can cause hearing loss.
| Danger area! Keep hands, fingers and arms away from this area.
| When transporting the power tool, hold it only at the locations indicated (recessed handles) or by the transport handle.
| When sawing bevel angles, the adjustable fences must be pulled outwards or removed completely.
| Take note of the dimensions of the saw blade (saw blade diameter D, hole diameter d). The hole diameter d must match the tool spindle without play. If it is necessary to use reducers, ensure that the dimensions of the reducer are suitable for the base blade thickness and the saw blade hole diameter, as well as the tool spindle diameter. Wherever possible, use the reducers provided with the saw blade. The saw blade diameter D must match the information specified on the symbol. See also: "Dimensions of suitable saw blades" in the "Technical Data" section.

## Asia/Africa/Latin America

The following symbols may be important for the operation of your power tool. Please take note of these symbols and their meaning. Correctly interpreting the symbols will help you to operate the power tool more effectively and safely.

Symbols and their meaning
| Laser radiation Do not look directly into the beam Laser class 2
| Keep hands away from the cutting area while the power tool is running. Contact with the saw blade can lead to injuries.
| Wear a dust mask.
| Wear safety goggles.
| Wear hearing protection. Exposure to noise can cause hearing loss.
| Danger area! Keep hands, fingers and arms away from this area.
| When transporting the power tool, hold it only at the locations indicated (recessed handles) or by the transport handle.
| When sawing bevel angles, the adjustable fences must be pulled outwards or removed completely.
| Take note of the dimensions of the saw blade (saw blade diameter D, hole diameter d). The hole diameter d must match the tool spindle without play. If it is necessary to use reducers, ensure that the dimensions of the reducer are suitable for the base blade thickness and the saw blade hole diameter, as well as the tool spindle diameter. Wherever possible, use the reducers provided with the saw blade. The saw blade diameter D must match the information specified on the symbol. See also: "Dimensions of suitable saw blades" in the "Technical Data" section.