# Product Features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Locking screw for slide device
(2) | Slide device
(3) | Transport handle
(4) | Protective guard
(5) | Lock-off function for on/off switch
(6) | On/off switch
(7) | Handle
(8) | Laser protection cap
(9) | Laser beam outlet aperture
(10) | Retracting blade guard
(11) | Guide roller
(12) | Saw table
(13) | Mounting holes
(14) | Insert plate
(15) | Locking clamp
(16) | Locking knob for various mitre angles
(17) | Mitre pre-setting lever
(18) | Tilt protector
(19) | Laser warning label
(20) | Detents for standard mitre angles
(21) | Scale for mitre angles
(22) | Clamping screw for saw table extension
(23) | Saw table extension
(24) | Workpiece support (flexibly pluggable)
(25) | Fixed fence
(26) | Adjustable fence
(27) | Scale for bevel angle
(28) | Angle indicator for bevel angles
(29) | Chip deflector
(30) | Saw blade
(31) | Spindle lock
(32) | Rechargeable battery release button
(33) | Rechargeable battery
(34) | Transport safety lock
(35) | Tilt protector
(36) | Length stop
(37) | Dust bag
(38) | Depth stop adjusting screw
(39) | Depth stop
(40) | Threaded rod
(41) | Screw clamp
(42) | Holes for screw clamp
(43) | Hex key/slotted screwdriver
(44) | Locking screw for the adjustable fence
(45) | Clamping wheel for bevel angle
(46) | Locking lever for bevel angle
(47) | Opening for workpiece support (on power tool)
(48) | Opening for second workpiece support (on workpiece support)
(49) | Threaded bolts
(50) | Dust extraction adapter
(51) | Hex socket screw for mounting the saw blade
(52) | Clamping flange
(53) | Inner clamping flange
(54) | Fastening screws for insert plate
(55) | Screw for laser protection cap
(56) | Fastening screw for laser housing
(57) | Laser housing
(58) | Angle indicator for mitre angles
(59) | Screw for mitre angle indicator
(60) | Screw for bevel angle indicator
(61) | Recessed handles