# Technical Data

Cordless sliding mitre saw |  | GCM 18V-216 D | GCM 18V-216 D
--- | --- | --- | ---
Article number |  | ‎ ‎3 601 M51 0..‎ | ‎ ‎3 601 M51 0B.‎ ‎ ‎3 601 M51 08.‎
Rated voltage | V= | 18 | 18
No-load speedA) | min–1 | 5000 | 5000
Laser type | nm | 650 | 650
| mW | < 1 | < 1
Laser class |  | 2 | 2
WeightB) | kg | 16.4–17.4 | 16.4–17.4
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50 | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V... | GBA 18V... ProCORE18V...
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36... | GAL 18... GAX 18... GAL 36...
Dimensions of suitable saw blades
Saw blade diameter D | mm | 216 | 216
Base blade thickness | mm | 1.2–1.8 | 1.2–1.8
Hole diameter d | mm | 30 | 25.4

A)

  Measured at 20–25 °C with rechargeable battery ProCORE18V 8.0Ah

B)

  Depends on battery in use

C)

  Limited performance at temperatures < 0 °C

Permitted workpiece dimensions (maximum/minimum): see Permissible workpiece dimensions

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.