# Operation

- Before carrying out any work on the power tool (e.g. maintenance, tool change etc.), remove the battery from the power tool. There is risk of injury from unintentionally pressing the on/off switch.

Transport safety lock
Preparing for operation
Adjusting mitre angles
Adjusting bevel angles
Start-up
Sawing
Practical advice
Adjusting the laser
Checking and Adjusting the Basic Settings
Transporting the Power Tool