# Adjusting mitre angles

- Bring the power tool into the work position.

## Setting Standard Mitre Angles (see figure H)

For quick and precise setting of commonly used mitre angles, detents (45) are provided on the saw table:

Left | Right
--- | ---
0°
45°; 30°; 22.5°; 15° | 15°; 22.5°; 30°; 45°

- Loosen the locking knob (11) if it is tightened.
- Pull the lever (12) and rotate the saw table (10) left or right to the required detent.
- Release the lever again. The lever must be felt to engage in the detent.
- Retighten the locking knob (11).

## Setting Any Mitre Angle (see figure H)

The mitre angle can be set between 47° (left-hand side) and 52° (right-hand side).

- Loosen the locking knob (11) if it is tightened.
- Push the lever (12), turn the saw table (10) left or right by the locking knob and set the required mitre angle using the angle indicator (13).
- Retighten the locking knob (11).