# Transport (see figure U)

Before transporting the power tool, the following steps must be carried out:

- Bring the power tool into the transport position.
- Remove all accessories that cannot be securely fitted to the power tool.
  If possible, transport unused saw blades in a closed container.
- Carry the power tool by the transport handle (3) or hold it by the recessed handles (26) on the sides of the saw table.

- Only use the transport devices to transport the power tool and never the protective devices.