# Start-up

- Pay attention to the mains voltage. The voltage of the power source must match the voltage specified on the rating plate of the power tool.

## Switching on (see figure J)

- To switch on the power tool, first slide the lock-off button (5) to the middle and then press and hold the on/off switch (19).

Note: For safety reasons, the on/off switch (19) cannot be locked; it must remain pressed during the entire operation.

## Switching off

- To switch off, release the on/off switch (19).