# Adjusting bevel angles

The bevel angle can be set between 45° (left-hand side) and 0° (right-hand side).

For quick and precise setting of frequently used bevel angles, fixed positions have been provided for the angles 0° and 45°.

## Setting Any Bevel Angle (see figure I)

- Loosen the clamping bolt (24).
- Use the handle (4) to swivel the tool arm until the angle indicator (30) shows the required bevel angle.
- Hold the tool arm in this position and retighten the clamping bolt (24).