# Transport Safety Lock (see figure D)

The transport safety lock (25) makes it easier to handle the power tool when transporting it to various working locations.

## Unlocking the power tool (work position)

- Press the tool arm down slightly by the handle (4) to release the transport safety lock (25).
- Pull the transport safety lock (25) all the way out.
- Slowly guide the tool arm upwards.

## Locking the power tool (transport position)

- To lock the saw table (10) in place, tighten the locking knob (11).
- Swing the tool arm downwards by the handle (4) until you can press the transport safety lock (25) all the way in.

The tool arm is now securely locked and ready for transportation.