# Operation

- Pull the plug out of the socket before carrying out any work on the power tool.

- Products that are only sold in AUS and NZ: Use a residual current device (RCD) with a nominal residual current of 30 mA or less.

Transport safety lock
Preparing for operation
Adjusting mitre angles
Adjusting bevel angles
Start-up
Sawing
Practical advice
Working on mouldings
Adjusting the laser
Checking and Adjusting the Basic Settings
Transport