# Product Features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Dust bag
(2) | Protective guard
(3) | Transport handle
(4) | Handle
(5) | Lock-off function for On/Off switch
(6) | Laser warning label
(7) | Retracting blade guard
(8) | Fence
(9) | Workpiece support (flexibly pluggable)
(10) | Saw table
(11) | Locking knob for all mitre angles
(12) | Mitre pre-setting lever
(13) | Angle indicator for mitre angles
(14) | Scale for mitre angles
(15) | Screw clamp
(16) | Folding fence
(17) | Guide roller
(18) | Chip deflector
(19) | On/off switch
(20) | On/Off switch for laser (cutting line indication)
(21) | Holes for screw clamp
(22) | Chip ejector
(23) | Mounting holes
(24) | Clamping bolt for all bevel angles
(25) | Transport safety lock
(26) | Recessed handles
(27) | Spindle lock
(28) | Hex key
(29) | Laser beam outlet aperture
(30) | Angle indicator for bevel angles
(31) | Scale for bevel angles
(32) | Guide rail for length gauge
(33) | Clamping screw for length stop
(34) | Wing bolt for fixing the guide rail for length gauge
(35) | Length stop
(36) | Insert plate
(37) | Hex socket screw for mounting the saw blade
(38) | Clamping flange
(39) | Saw bladeA)
(40) | Inner clamping flange
(41) | Wing bolt for adjusting the height of the threaded rod
(42) | Threaded rod
(43) | Wing bolt for screw clamp
(44) | Screw clamp pins
(45) | Detents for standard mitre angles
(46) | Screws for insert plate
(47) | Set screw for positioning the laser
(48) | Set square
(49) | Hex socket screw for fence
(50) | Stop screw for 0° bevel angle
(51) | Stop screw for 45° bevel angle
(52) | Screw for bevel angle indicator
(53) | Screw for mitre angle indicator

A)

  This accessory is not part of the standard scope of delivery.