# Product Features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Locking screw for slide device
(2) | Slide device
(3) | Laser warning label
(4) | Transport handle
(5) | Handle
(6) | Lock-off function for On/Off switch
(7) | Protective guard
(8) | Retracting blade guard
(9) | Mounting holes
(10) | Insert plate
(11) | Lock button for mitre angle
(12) | Locking knob for all mitre angles
(13) | Lock button for bevel angle
(14) | Angle indicator for mitre angles
(15) | Detents for standard mitre angles
(16) | Saw table extension
(17) | Workpiece supportA)
(18) | Fixed fence
(19) | Adjustable fence
(20) | Screw clamp
(21) | Adjustment knob for 0° bevel angle
(22) | Depth stop
(23) | Depth stop adjusting screw
(24) | Hex key
(25) | Transport Safety Lock
(26) | Length stop
(27) | Recessed handles
(28) | Mounting holes for horizontal fixing
(29) | Saw table
(30) | Scale for mitre angles
(31) | Tilt protector
(32) | Guide roller
(33) | Spindle lock
(34) | Laser beam outlet aperture
(35) | On/off switch
(36) | On/Off switch for laser (cutting line indication)
(37) | Chip ejector
(38) | Wing bolt for fixing the adjustable fence
(39) | Holes for screw clamp
(40) | Stop screw for right-hand bevel angle range
(41) | Standard bevel angle stops 45°, 22.5° and 33.9°
(42) | Clamping screw for saw table extension
(43) | Securing screw for saw table extension
(44) | Opening for workpiece support (on power tool)
(45) | Opening for second workpiece support (on workpiece support)
(46) | Dust bag
(47) | Hex socket screw for mounting the saw blade
(48) | Clamping flange
(49) | Saw blade
(50) | Inner clamping flange
(51) | Wing bolt for adjusting the height of the threaded rod
(52) | Threaded rod
(53) | Wing bolt for screw clamp
(54) | Screw clamp pins
(55) | Angle indicator for bevel angles
(56) | Scale for bevel angles
(57) | Clamping screw for length stop
(58) | Guide rail for length gauge
(59) | Wing bolt for fixing the guide rail for length gauge
(60) | Screws for insert plate
(61) | Set screw for positioning the laser
(62) | Set square
(63) | Stop screw for 0° bevel angle
(64) | Hex socket screw for fence
(65) | Screw for bevel angle indicator
(66) | Screw for mitre angle indicator

A)

  Not available in all country-specific versions.