# Changing the saw blade (see figures D1−D4)

- Pull the plug out of the socket before carrying out any work on the power tool.

- Wear protective gloves when fitting the saw blade. There is a risk of injury when touching the saw blade.

Only use saw blades that have a maximum permitted speed higher than the no-load speed of the power tool.

Only use saw blades that match the specifications given in this operating manual and that have been tested and marked in accordance with EN 847-1.

Only use saw blades that are recommended by the power tool manufacturer and are suitable for use on the material you want to saw. This will prevent the saw teeth overheating when sawing.

## Removing the Saw Blade

- Bring the power tool into the work position.
- Swivel the retracting blade guard (8) to the back and hold it in this position.
- Turn the hex socket screw (47) with the hex key (8 mm) (24) and at the same time push the spindle lock (33) until it engages.
- Keep holding the spindle lock (33) and loosen the hex socket screw (47) by turning it clockwise (left-hand thread).
- Remove the clamping flange (48).
- Remove the saw blade (49).
- Slowly push the retracting blade guard back down.

## Fitting the saw blade

- When fitting the saw blade, make sure that the cutting direction of the teeth (arrow direction on the saw blade) matches the direction of the arrow on the protective guard.

If required, clean all the parts you want to fit before installing them.

- Swivel the retracting blade guard (8) to the back and hold it in this position.
- Place the new saw blade on the inner clamping flange (50).

- Fit the clamping flange (48) and the hex socket screw (47). Press the spindle lock (33) until it engages and tighten the hex socket screw by turning it anticlockwise.
- Slowly push the retracting blade guard back down.