# Symbols

## Europe

The following symbols may be important for the operation of your power tool. Please take note of these symbols and their meaning. Correctly interpreting the symbols will help you to operate the power tool more effectively and safely.

Symbols and their meaning
| Laser radiation Do not look directly into the beam Class 2 consumer laser product EN 50689:2021
| Keep hands away from the cutting area while the power tool is running. Contact with the saw blade can lead to injuries.
| Wear a dust mask.
| Wear safety goggles.
| Wear hearing protection. Exposure to noise can cause hearing loss.
| Danger area! Keep hands, fingers and arms away from this area.
| To set any bevel angle, the tool arm must be able to move freely. Lock button pulled up: The bevel angle can be set. Lock button pushed down: The set bevel angle is locked.
| Take note of the dimensions of the saw blade. The hole diameter must match the tool spindle without play. If it is necessary to use reducers, ensure that the dimensions of the reducer are suitable for the base blade thickness and the saw blade hole diameter, as well as the tool spindle diameter. Wherever possible, use the reducers provided with the saw blade. The saw blade diameter must match the information specified on the symbol.
| The left/right adjustable fence must be removed when sawing bevel angles.

## Asia/Africa

The following symbols may be important for the operation of your power tool. Please take note of these symbols and their meaning. Correctly interpreting the symbols will help you to operate the power tool more effectively and safely.

Symbols and their meaning
| Laser radiation Do not look directly into the beam Laser class 2
| Keep hands away from the cutting area while the power tool is running. Contact with the saw blade can lead to injuries.
| Wear a dust mask.
| Wear safety goggles.
| Wear hearing protection. Exposure to noise can cause hearing loss.
| Danger area! Keep hands, fingers and arms away from this area.
| To set any bevel angle, the tool arm must be able to move freely. Lock button pulled up: The bevel angle can be set. Lock button pushed down: The set bevel angle is locked.
| Take note of the dimensions of the saw blade. The hole diameter must match the tool spindle without play. If it is necessary to use reducers, ensure that the dimensions of the reducer are suitable for the base blade thickness and the saw blade hole diameter, as well as the tool spindle diameter. Wherever possible, use the reducers provided with the saw blade. The saw blade diameter must match the information specified on the symbol.
| The left/right adjustable fence must be removed when sawing bevel angles.