# Technical Data

## Europe

Sliding Mitre Saw |  | GCM 254 D
--- | --- | ---
Article number |  | ‎ ‎3 601 M53 0..‎
Rated power input | W | 1800
No-load speed | min–1 | 4800
Laser type | nm | 650
| mW | < 1
Laser class |  | 2
Weight | kg | 17.9
Protection class |  | / II
Dimensions of suitable saw blades
Saw blade diameter | mm | 254
Base blade thickness | mm | 1.4–2.5
Max. cutting width | mm | 3
Hole diameter | mm | 30

Permitted workpiece dimensions (maximum/minimum): see Permissible workpiece dimensions

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

The appliance meets IEC 61000-3-11 requirements and is subject to conditional connection. The appliance can lead to occasional voltage fluctuations under unfavorable power conditions. The impedance of this appliance is set as Zactual = 0.094 Ω. The user must make sure, that the connection point, with the impedance Zmax, on which the appliance shall be plugged in meets the impedance requirement: Zactual ≥ Zmax. If Zmax is unknown, determine Zmax in consultation with the network supplier or supply authority.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.

## Asia/Africa

Sliding Mitre Saw |  | GCM 254 D
--- | --- | ---
Article number |  | ‎ ‎3 601 M53 0..‎
Rated power input | W | 1800
No-load speed | min–1 | 4800
Laser type | nm | 650
| mW | < 1
Laser class |  | 2
Weight | kg | 17.9
Protection class |  | / II
Dimensions of suitable saw blades
Saw blade diameter | mm | 254
Base blade thickness | mm | 1.4–2.5
Max. cutting width | mm | 3
Hole diameter | mm | 25.4

Permitted workpiece dimensions (maximum/minimum): see Permissible workpiece dimensions

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

The appliance meets IEC 61000-3-11 requirements and is subject to conditional connection. The appliance can lead to occasional voltage fluctuations under unfavorable power conditions. The impedance of this appliance is set as Zactual = 0.094 Ω. The user must make sure, that the connection point, with the impedance Zmax, on which the appliance shall be plugged in meets the impedance requirement: Zactual ≥ Zmax. If Zmax is unknown, determine Zmax in consultation with the network supplier or supply authority.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.