# Start-up

- Pay attention to the mains voltage. The voltage of the power source must match the voltage specified on the rating plate of the power tool.

- Always firmly tighten the locking knob (12) and push the lock button down (13) before sawing. Otherwise the saw blade can become wedged in the workpiece.

## Switching on (see figure L)

- To start the power tool, first press the lock-off button (6). Then press the on/off switch (35) all the way in and keep it pressed.

Note: For safety reasons, the on/off switch (35) cannot be locked; it must remain pressed during the entire operation.

## Switching off

- To switch off, release the on/off switch (35).