# Fitting individual components

- Carefully remove all parts included in the delivery from their packaging.
- Remove all packing material from the power tool and the accessories provided.

- For ease of assembly when fitting the tool elements that are provided, be aware that the power tool is supplied in the transport position.

## Fitting the saw table extensions (see figure A1)

To extend the saw table further, saw table extensions can be mounted both to the left or right of the power tool.

- Unscrew the securing screws (43) from the saw table extensions with a cross-headed screwdriver.
- Tilt the power tool.
- Push the saw table extensions (16) on both sides of the power tool all the way into the corresponding drill holes.
- For the pull-out safety device, screw the securing screws (43) back into the saw table extensions.

## Installing Workpiece Supports (see figure A2)

The workpiece supports (17) can be positioned left, right or in front of the power tool. The flexible connector system enables a multitude of extension or expansion variants (see figure G).

- Insert the workpiece support (17) into the openings (44) on the power tool or into the openings (45) of the second workpiece support as required.

- Never carry the power tool using the workpiece supports.
  Only use the transport devices to transport the power tool.