# Adjusting mitre angles

- Bring the power tool into the work position.

## Setting Standard Mitre Angles (see figure J)

For quick and precise setting of commonly used mitre angles, detents (15) are provided on the saw table:

Left | Right
--- | ---
0°
45°; 22.5°; 15° | 15°; 22.5°; 45°

- Loosen the locking knob (12) if it is tightened.
- Press the lock button (11) down and turn the saw table (29) left or right by the locking knob until the angle indicator (14) shows the standard mitre angle required.
- Release the lock button (11) again. The saw table must be heard to click into the detent.
- Retighten the locking knob (12).

## Setting any Mitre Angle

The mitre angle can be set between 47° (left-hand side) and 52° (right-hand side).

- Loosen the locking knob (12) if it is tightened.
- Press the lock button (11) down and turn the saw table (29) left or right by the locking knob until the angle indicator (14) shows the mitre angle required.
- Release the lock button (11) again.
- Retighten the locking knob (12).