# Transporting the Power Tool (see figure Y)

Before transporting the power tool, the following steps must be carried out:

- Loosen the locking screw (1) if it is tightened. Pull the tool arm fully forwards and retighten the locking screw.
- Make sure that the depth stop (22) is pressed all the way in and that the adjusting screw (23) fits through the recess without touching the depth stop when moving the tool arm.
- Bring the power tool into the transport position.
- Remove all accessories that cannot be securely fitted to the power tool. If possible, transport unused saw blades in an enclosed container.
- Carry the power tool by the transport handle (4) or hold it by the recessed handles (27) on the sides of the saw table.

- Only use the transport devices to transport the power tool and never the protective devices or workpiece supports.