# Adjusting bevel angles

The bevel angle can be set between 45° (left-hand side) and 45° (right-hand side).

For quick and precise setting of frequently used bevel angles, stops have been provided for the angles 0°, 22.5°, 33.9° and 45°.

##

- Remove the left-hand adjustable fence (19)
- Turn the left-hand stop (41) until the standard 45° bevel angle engages at the arrow mark.
  The full swivel range to the left is now available.
- Pull the lock button (13) up.
- Use the handle (5) to swivel the tool arm to the left until the angle indicator shows the required bevel angle.
- Hold the tool arm in this position and push the lock button (13) back down.

##

- Remove the right adjustable fence (19).
- Turn the right-hand stop (41) until the standard 45° bevel angle engages at the arrow mark.
  The right swivel range to the right is now available.
- Pull the lock button (13) up.
- Turn the adjustment knob (21) slightly to the left and swivel the tool arm to the right by the handle (5) until the angle indicator shows the required bevel angle.
- Hold the tool arm in this position and push the lock button (13) back down.

##

- Remove the right/left adjustable fence (19).
- Pull the lock button (13) up.

Standard mitre angle 0°:

- Turn the adjustment knob (21) slightly to the left and swivel the tool arm from the right to the 0° position until you hear it click into place in the 0° position.
- Push the lock button (13) back down.

Standard mitre angles 45°, 33.9° and 22.5°:

- Turn the left-hand or right-hand stop (41) until the required standard bevel angle engages at the arrow mark.
- Swivel the tool arm as far as it will go to the left.
  or
  Turn the adjustment knob (21) slightly to the left and swivel the tool arm to the right by the handle (5) as far as it will go.
- Push the lock button (13) back down.