# Technical Data

Cordless glue gun |  | AdvancedGlue 18V
--- | --- | ---
Article number |  | ‎3 603 B64 8..‎‎‎‎
Rated voltage | V= | 18
Heat-up time approx.A) | min | 2
Gluing temperature (can be selected) | °C °C | 130 200
Max. gluing capacity | g/min | 20
Glue stick
Diameter | mm | 11
Length | mm | 45−200
Operating timeA) per battery charge up to |  | 10 glue sticks
Weight according to EPTA-Procedure 01:2014B) | kg | 0.68−0.99
Permitted ambient temperature |  |
During charging | °C | 0 to +35
During operation and during storage | °C | +5 to +40
Recommended rechargeable batteries |  | PBA 18V...W-.
Recommended battery chargersC) |  | AL 18...

A)

  Measured at 20–25 °C with battery PBA 18V 2.5Ah W-. and processing temperature 200 °C.

B)

  Depends on battery in use

C)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV