# Starting Operation

## Switching On and Off

- To switch on the glue gun, press the on/off button (8).
  The glue gun heats to the last set processing temperature (130 °C or 200 °C).
  The relevant temperature selection button (7) or (9) will flash green while the tool is heating up. Once it is continuously lit green, the glue gun is ready to use.

If you change the processing temperature during operation, the relevant temperature selection button (7) or (9) will flash green until the target temperature required is reached. The cooling process from 200 °C to 130 °C may take several minutes.

- To switch off the glue gun, press and hold the on/off button (8) until the LED for the relevant temperature selection button (7) or (9) goes out.

Note: If the glue gun is not used for longer than 10 minutes, it will switch off automatically to save energy.

- If the temperature selection button (7) or (9) lights up red continuously after switching on again, you must charge the battery.

- Safely place the glue gun down after use and let it cool completely before packing it away. The hot nozzle can cause damage.