# Maintenance and Cleaning

- Warning! Switch the glue gun off before commencing maintenance and cleaning work.

- Keep the glue gun clean to ensure effective, safe operation.

After the adhesive has hardened, you can remove it with a blunt object. Do not use solvents when cleaning. If necessary, the bonding locations can be unstuck again by applying heat.

An inserted glue stick (3) must not be removed from the rear of the glue gun. This is to prevent damage to the glue gun.