# Technical Data

Cordless tacker |  | UniversalTacker 18V-14
--- | --- | ---
Article number |  | ‎3 603 BA7 0..
Impact rate | min−1 | 30
Fasteners
Staple strip |  | Type 53
Width | mm | 11.4
Length | mm | 6–14
Nail strip |  | Type 48
Length | mm | 14
Max. magazine capacity |  | 140
Weight according to EPTA-Procedure 01:2014A) | kg | 1.8 (1.5 Ah)–2.1 (6.0 Ah)
Permitted ambient temperature |  |
During charging | °C | 0 to +35
During operationB) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | PBA 18V...W-.
Recommended battery chargersC) |  | AL 18...

A)

  Depends on battery in use

B)

  Limited performance at temperatures < 0 °C

C)

  The following chargers are not compatible with the PBA rechargeable battery: AL 1814 CV, AL 1820 CV, AL 1860 CV