# Loading the Magazine (see figures A1–A2)

- Use only original Bosch accessories. The precision parts of the tacker, such as the magazine, striker and shot duct, are matched to Bosch staples and nails. Other manufacturers use different steel grades and sizes.

The viewing window of the refill indicator (11) indicates whether there are any remaining staples or nails in the magazine.

- Turn the power tool around.
- Press the magazine release (8) and pull the magazine (9) out of the back of the tool at the same time.
- Insert the staple strip (14) or nail strip (15).
  When inserting the nail strip (15), hold the tacker slightly at an angle so that the nails lie flat on the side wall. Note the marking.
- Slide the magazine (9) back in until it clicks into place.

- Do not use force when opening, loading or closing the magazine.