# Loading the Magazine (see figures A1–A3)

- Use only original Bosch accessories. The precision parts of the tacker, such as the magazine, striker and shot duct, are matched to Bosch staples and nails. Other manufacturers use different steel grades and sizes.

The viewing window of the refill indicator (23) indicates whether there are any remaining staples or nails in the magazine.

- Place the power tool on a flat surface.
- Press the magazine release (13) and pull the magazine (12) out of the back of the tool at the same time.
- Insert the staple strip (20) or nail strip (21).
  Note: When inserting nails or staples, pay attention to the different insertion positions (see figures A2–A3). Nails are applied to the lower edge of the magazine (see figure A2). Staples are applied to the upper edge of the magazine (see figure A3). Push the nails or staples all the way to the front after inserting them in the magazine. Note the marking.
- Slide the magazine (12) back in until it clicks into place.

- Do not use force when opening, loading or closing the magazine.